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	Install XPS260M to Windows

	+ You must install the printer on Windows before following these steps
+ Follow the included help sheet titled Windows USB Installation
+ Alternatively, go to cashregistergroup.co.uk/faq#/Printers/XPS260M



	Open Print Options
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	Open Aronium
	Press MENU
	Press SETTINGS
	Press PRINT OPTIONS



	Enable Printing
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	Enable PRINT RECEIPT
	Select XP-80C
	Open PRINTER SETTINGS



	Configure Printer Settings
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	Set Printer Type
	Set Margins
	Set Cash Drawer

	Set printer type to POS 80, this enables the printer to print graphic receipts
	Set the right margin to 8, this ensures that the print will not be cut off on the right
	Ensure OPEN CASH DRAWER is enabled, input the command 27,112,0,148,49



	Test and Save
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	Test Print
	Test Drawer
	Save Settings
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